PLUVIAL FLOODS INPUT LAYERS

1. **BASINS**
2. Extract Europe basins which intersect with specific city boundary
3. **STREAMS**
4. Extract Europe streams which intersect with specific city boundary
5. Extract specific Digital Elevation Model area intersecting city boundary
6. Assign DEM altitude values to start and end points of each stream